| Routines

F5FB: Guide a character from one spot on the sidewalk or road to another

The address of this interruptible subcommand routine is placed into bytes 0x0E and 0x0F of a character's buffer by the routine at F600. It guides the character left or right over the sidewalk or road towards his destination.
Input
H | Character number (0xD7-0xE5)
F5FB | LD BC,$F5EE | Point BC at the RET instruction at F5EE
F5FE | JR $F5D1 | Move the character left or right towards his destination