| Routines

63128: Check whether a character is midstride

Used by the routines at 29361, 31362, 62976 and 63209. Returns to the caller unless the character is midstride; otherwise moves the character from the midstride position and returns to the routine at 61948 to move the next character.
Input
H | Character number (215-229)
63128 | LD L,0 | Point HL at byte 0 of the character's buffer
This entry point is used by the routine at 63118.
63130 | BIT 0,(HL) | Is the character midstride?
63132 | RET Z | Return if not
63133 | POP BC | Drop the return address from the stack
63134 | JP 60506 | Move the character from the midstride position and update the SRB