| Unused

6C82: Unused

If messages 0x82-0xC7 existed, these bytes would be the LSBs of their addresses. The corresponding unused MSBs can be found at 6D82.
6C82 | DEFB $FE,$FE,$FE,$FE,$FE,$FE |
6C88 | DEFB $FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE |
6C98 | DEFB $FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE |
6CA8 | DEFB $FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE |
6CB8 | DEFB $FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE,$FE |