| Routines

64582: Generate the table of mirrored values of 0-255

Used by the routines at 63662 and 64618. Generates the table of mirrored values of 0-255 at 32256.
64582 | LD HL,32256 | Point HL at the first slot in the table
64585 | LD A,L | A=byte that will be mirrored
64586 | LD BC,2048 | B=8, C=0
64589 | RLCA | Generate the mirror byte in C
64590 | RR C
64592 | DJNZ 64589
64594 | LD (HL),C | Store the mirror byte
64595 | INC L | Point HL at the next slot in the table
64596 | JR NZ,64585 | Jump back until the table is complete
64598 | RET |