| Unused

A716: Unused

The first two bytes here may once have been used as the address of a special location handler routine, which would have been invoked by a three-byte special location descriptor with 8 as the third byte (such as the unused three-byte location descriptor in the table at C24E). The addresses of the special location handler routines that are used can be found at A016, A116, A216, A316, A416, A516 and A616.
A716 | DEFB $0A,$73 |
A718 | DEFB $00,$00,$00,$00 |