| Messages

02465: THE CASSETTE MESSAGES

Used by the routines at SAVE_ETC and SA_CONTRL. Each message is given with the last character inverted (plus 128).
CASSETTE | 02465 | DEFB 128 | Initial byte is stepped over.
| 02466 | DEFM "Start tape, then press any key","."+128 | 'Start tape, then press any key.'
BLOCK_HDR | 02497 | DEFM 13,"Program:"," "+128 | Carriage return + 'Program: '
| 02507 | DEFM 13,"Number array:"," "+128 | Carriage return + 'Number array: '
| 02522 | DEFM 13,"Character array:"," "+128 | Carriage return + 'Character array: '
| 02540 | DEFM 13,"Bytes:"," "+128 | Carriage return + 'Bytes: '