| Routines

07091: THE 'LINE-END' ROUTINE

Used by the routines at STMT_LOOP, STMT_NEXT and IF_CMD. The routine at REM continues here. If checking syntax a simple return is made but when 'running' the address held by NXTLIN has to be checked before it can be used.
LINE_END | 07091 | CALL SYNTAX_Z | Return if syntax is being checked; otherwise fetch the address in NXTLIN.
| 07094 | RET Z
| 07095 | LD HL,(23637)
| 07098 | LD A,192 | Return also if the address is after the end of the program - the 'run' is finished.
| 07100 | AND (HL)
| 07101 | RET NZ
| 07102 | XOR A | Signal 'statement zero' before proceeding.
This routine continues into LINE_USE.