| Routines

107F: THE 'ED-ERROR' SUBROUTINE

Used by the routine at EDITOR. Come here when there has been some kind of error.
ED_ERROR | 107F | BIT 4,(IY+$30) | Jump back if using other than channel 'K' (bit 4 of FLAGS2 reset).
| 1083 | JR Z,ED_END
| 1085 | LD (IY+$00),$FF | Cancel the error number (ERR-NR) and give a 'rasp' (see RASP) before going around the editor again.
| 1089 | LD D,$00
| 108B | LD E,(IY-$02)
| 108E | LD HL,$1A90
| 1091 | CALL BEEPER
| 1094 | JP ED_AGAIN