| Routines

2AEE: THE 'DE,(DE+1)' SUBROUTINE

Used by the routine at STK_VAR. This subroutine performs the construction 'LD DE,(DE+1)' and returns HL pointing to 'DE+2'.
Input
DE | Target address minus one
Output
DE | Word at the target address
HL | Target address plus one
DE_DE_1 | 2AEE | EX DE,HL | Use HL for the construction.
| 2AEF | INC HL | Point to 'DE+1'.
| 2AF0 | LD E,(HL) | In effect - LD E,(DE+1).
| 2AF1 | INC HL | Point to 'DE+2'.
| 2AF2 | LD D,(HL) | In effect - LD D,(DE+2).
| 2AF3 | RET | Finished.