| Routines

04083: THE 'CURSOR DOWN EDITING' SUBROUTINE

The address of this routine is derived from an offset found in the editing keys table.
ED_DOWN | 04083 | BIT 5,(IY+55) | Jump forward if in 'INPUT mode' (bit 5 of FLAGX set).
| 04087 | JR NZ,ED_STOP
| 04089 | LD HL,23625 | This is E-PPC.
| 04092 | CALL LN_FETCH | The next line number is found and a new automatic listing produced.
| 04095 | JR ED_LIST
ED_STOP | 04097 | LD (IY+0),16 | 'STOP in INPUT' report (ERR-NR).
| 04101 | JR ED_ENTER | Jump forward.