| Routines

08662: THE 'IN-CHAN-K' SUBROUTINE

Used by the routine at INPUT.
Output
F | Zero flag set if channel 'K' (keyboard) is being used
IN_CHAN_K | 08662 | LD HL,(23633) | The base address of the channel information for the current channel (CURCHL) is fetched and the channel code compared to the character 'K'.
| 08665 | INC HL
| 08666 | INC HL
| 08667 | INC HL
| 08668 | INC HL
| 08669 | LD A,(HL)
| 08670 | CP "K"
| 08672 | RET | Return afterwards.