| Routines

07050: THE 'LINE-RUN' ENTRY POINT

Used by the routine at MAIN_EXEC. The routine at STMT_RET continues here. This entry point is used wherever a line in the editing area is to be 'run'. In such a case the syntax/run flag (bit 7 of FLAGS) will be set. The entry point is also used in the syntax checking of a line in the editing area that has more than one statement (bit 7 of FLAGS will be reset).
LINE_RUN | 07050 | LD HL,65534 | A line in the editing area is considered as line '-2'; set PPC accordingly
| 07053 | LD (23621),HL
| 07056 | LD HL,(23649) | Make HL point to the end marker of the editing area (WORKSP-1) and DE to the location before the start of that area (E-LINE-1).
| 07059 | DEC HL
| 07060 | LD DE,(23641)
| 07064 | DEC DE
| 07065 | LD A,(23620) | Fetch the number of the next statement to be handled (NSPPC) before jumping forward.
| 07068 | JR NEXT_LINE