| Routines

05606: THE 'INPUT-AD' SUBROUTINE

Used by the routines at WAIT_KEY and read_in. The registers are saved and HL made to point to the input address.
INPUT_AD | 05606 | EXX | Save the registers.
| 05607 | PUSH HL
| 05608 | LD HL,(23633) | Fetch the base address for the current channel information (CURCHL).
| 05611 | INC HL | Step past the output address.
| 05612 | INC HL
| 05613 | JR CALL_SUB | Jump forward.