| Routines

04223: THE 'ED-ERROR' SUBROUTINE

Used by the routine at EDITOR. Come here when there has been some kind of error.
ED_ERROR | 04223 | BIT 4,(IY+48) | Jump back if using other than channel 'K' (bit 4 of FLAGS2 reset).
| 04227 | JR Z,ED_END
| 04229 | LD (IY+0),255 | Cancel the error number (ERR-NR) and give a 'rasp' (see RASP) before going around the editor again.
| 04233 | LD D,0
| 04235 | LD E,(IY-2)
| 04238 | LD HL,6800
| 04241 | CALL BEEPER
| 04244 | JP ED_AGAIN