| Routines

0FF3: THE 'CURSOR DOWN EDITING' SUBROUTINE

The address of this routine is derived from an offset found in the editing keys table.
ED_DOWN | 0FF3 | BIT 5,(IY+$37) | Jump forward if in 'INPUT mode' (bit 5 of FLAGX set).
| 0FF7 | JR NZ,ED_STOP
| 0FF9 | LD HL,$5C49 | This is E-PPC.
| 0FFC | CALL LN_FETCH | The next line number is found and a new automatic listing produced.
| 0FFF | JR ED_LIST
ED_STOP | 1001 | LD (IY+$00),$10 | 'STOP in INPUT' report (ERR-NR).
| 1005 | JR ED_ENTER | Jump forward.