| Routines

05684: THE 'CHANNEL 'K' FLAG' SUBROUTINE

The address of this routine is derived from an offset found in the channel code lookup table.
CHAN_K | 05684 | SET 0,(IY+2) | Signal 'using lower screen' (set bit 0 of TV-FLAG).
| 05688 | RES 5,(IY+1) | Signal 'ready for a key' (reset bit 5 of FLAGS).
| 05692 | SET 4,(IY+48) | Signal 'using channel 'K'' (set bit 4 of FLAGS2).
| 05696 | JR CHAN_S_1 | Jump forward.