| Messages

09A1: THE CASSETTE MESSAGES

Used by the routines at SAVE_ETC and SA_CONTRL. Each message is given with the last character inverted (plus +80).
CASSETTE | 09A1 | DEFB $80 | Initial byte is stepped over.
| 09A2 | DEFM "Start tape, then press any key","."+$80 | 'Start tape, then press any key.'
BLOCK_HDR | 09C1 | DEFM $0D,"Program:"," "+$80 | Carriage return + 'Program: '
| 09CB | DEFM $0D,"Number array:"," "+$80 | Carriage return + 'Number array: '
| 09DA | DEFM $0D,"Character array:"," "+$80 | Carriage return + 'Character array: '
| 09EC | DEFM $0D,"Bytes:"," "+$80 | Carriage return + 'Bytes: '