| Routines

2045: THE 'END OF PRINTING' SUBROUTINE

Used by the routines at PRINT_2 and PR_POSN_1. The zero flag will be set if no further printing is to be done.
Input
A | Code of the current character
Output
F | Zero flag set if the character is ')', ':' or a carriage return
PR_END_Z | 2045 | CP ")" | Return now if the character is a ')'.
| 2047 | RET Z
This entry point is used by the routine at SAVE_ETC.
PR_ST_END | 2048 | CP $0D | Return now if the character is a 'carriage return'.
| 204A | RET Z
| 204B | CP ":" | Make a final test against ':' before returning.
| 204D | RET