| Routines

11560: THE 'STACK-A' SUBROUTINE

Used by the routines at POINT_SUB, DRAW, CD_PRMS1, S_ATTR_S, peek, code and ln. The routine at STK_DIGIT continues here. This subroutine gives the floating-point form for the absolute binary value currently held in the A register.
Input
A | Value to stack
STACK_A | 11560 | LD C,A | Transfer the value to the C register.
| 11561 | LD B,0 | Clear the B register.
This routine continues into STACK_BC.