| System variables

23658: FLAGS2 - More flags

Read by the routines at K_DECODE, ED_ERROR, MAIN_EXEC, OUT_CURS, OUT_SP_2 and INPUT, and updated by the routines at PO_ANY, CL_ALL, CLEAR_PRB, KEY_INPUT, CHAN_FLAG, CHAN_K, AUTO_LIST and OUT_LINE. This system variable is accessed by most routines via the IY register at IY+48.
Bit | Description
--- | ---
0 | Reset when the screen is clear
1 | Set when the printer buffer is in use
2 | Set when in quotes during line parsing
3 | Set when CAPS LOCK is on
4 | Set when using channel K (keyboard)
5 | Unused
6 | Unused
7 | Unused
FLAGS2 | 23658 | DEFB 0 |