| System variables

5C10: STRMS - Addresses of channels attached to streams

Initialised by the routine at NEW (from the initial stream data table), and read by the routines at CHAN_OPEN and STR_DATA. Each of these values is an offset that is added to the base address of the channel data (stored at CHANS) to find the corresponding entry in the channel information table (CHINFO).
STRMS | 5C10 | DEFW $0001 | Stream +FD (keyboard).
| 5C12 | DEFW $0006 | Stream +FE (screen).
| 5C14 | DEFW $000B | Stream +FF (work space).
| 5C16 | DEFW $0001 | Stream +00 (keyboard).
| 5C18 | DEFW $0001 | Stream +01 (keyboard).
| 5C1A | DEFW $0006 | Stream +02 (screen).
| 5C1C | DEFW $0010 | Stream +03 (printer).
| 5C1E | DEFW $0000 | Stream +04.
| 5C20 | DEFW $0000 | Stream +05.
| 5C22 | DEFW $0000 | Stream +06.
| 5C24 | DEFW $0000 | Stream +07.
| 5C26 | DEFW $0000 | Stream +08.
| 5C28 | DEFW $0000 | Stream +09.
| 5C2A | DEFW $0000 | Stream +0A.
| 5C2C | DEFW $0000 | Stream +0B.
| 5C2E | DEFW $0000 | Stream +0C.
| 5C30 | DEFW $0000 | Stream +0D.
| 5C32 | DEFW $0000 | Stream +0E.
| 5C34 | DEFW $0000 | Stream +0F.