| Routines

1B76: THE 'STMT-RET' SUBROUTINE

Used by the routine at STMT_LOOP. After the correct interpretation of a statement a return is made to this entry point.
STMT_RET | 1B76 | CALL BREAK_KEY | The BREAK key is tested after every statement.
| 1B79 | JR C,STMT_R_1 | Jump forward unless it has been pressed.
Report L - BREAK into program.
| 1B7B | RST $08 | Call the error handling routine.
| 1B7C | DEFB $14
Continue here as the BREAK key was not pressed.
STMT_R_1 | 1B7D | BIT 7,(IY+$0A) | Jump forward if there is not a 'jump' to be made (NSPPC is +FF).
| 1B81 | JR NZ,STMT_NEXT
| 1B83 | LD HL,($5C42) | Fetch the 'new line' number (NEWPPC) and jump forward unless dealing with a further statement in the editing area.
| 1B86 | BIT 7,H
| 1B88 | JR Z,LINE_NEW
This routine continues into LINE_RUN.