| Routines

26941: Print a speech bubble UDG

Used by the routine at 26958.
Input
DE | UDG address
HL | Attribute file address
26941 | PUSH HL | Save the attribute file address temporarily
26942 | LD (HL),56 | INK 0: PAPER 7
26944 | LD A,H | Set HL to the corresponding display file address
26945 | AND 11
26947 | ADD A,A
26948 | ADD A,A
26949 | ADD A,A
26950 | LD H,A
26951 | EX DE,HL |
26952 | CALL 24869 | Copy the speech bubble UDG onto the screen
26955 | EX DE,HL |
26956 | POP HL | Restore the attribute file address to HL
26957 | RET |