| Data

D33C: LSBs of addresses of ERIC-handling routines

Used by the routine at F7AD. The corresponding MSBs can be found at D43C.
D33C | DEFB $8E | LSB of F28E (used when bit 7 is set at 7FFB)
D33D | DEFB $00 | Unused (when bit 6 is set at 7FFB, ERIC is incapacitated)
D33E | DEFB $AD | LSB of 5EAD (used when bit 5 is set at 7FFB)
D33F | DEFB $6F | LSB of 5E6F (used when bit 4 is set at 7FFB)
D340 | DEFB $45 | LSB of E145 (used when bit 3 is set at 7FFB)
D341 | DEFB $E2 | LSB of F2E2 (used when bit 2 is set at 7FFB)
D342 | DEFB $00 | Unused (when bit 1 is set at 7FFB, ERIC's secondary status flags at 7FED are checked)
D343 | DEFB $63 | LSB of 5D63 (used when bit 0 is set at 7FFB)