| Data

D53C: LSBs of addresses of ERIC-handling routines

Used by the routine at F7AD. The corresponding MSBs can be found at D63C.
D53C | DEFB $16 | LSB of 7316 (used when bit 7 is set at 7FED)
D53D | DEFB $23 | LSB of 5D23 (used when bit 6 is set at 7FED)
D53E | DEFB $33 | LSB of 5D33 (used when bit 5 is set at 7FED)
D53F | DEFB $CC | LSB of FBCC (used when bit 4 is set at 7FED)
D540 | DEFB $A0 | LSB of FBA0 (used when bit 3 is set at 7FED)
D541 | DEFB $03 | LSB of FB03 (used when bit 2 is set at 7FED)
D542 | DEFB $3C | LSB of FB3C (used when bit 1 is set at 7FED)
D543 | DEFB $5E | LSB of 725E (used when bit 0 is set at 7FED)