| Data

54844: MSBs of addresses of ERIC-handling routines

Used by the routine at 63405. The corresponding LSBs can be found at 54588.
54844 | DEFB 115 | MSB of 29462 (used when bit 7 is set at 32749)
54845 | DEFB 93 | MSB of 23843 (used when bit 6 is set at 32749)
54846 | DEFB 93 | MSB of 23859 (used when bit 5 is set at 32749)
54847 | DEFB 251 | MSB of 64460 (used when bit 4 is set at 32749)
54848 | DEFB 251 | MSB of 64416 (used when bit 3 is set at 32749)
54849 | DEFB 251 | MSB of 64259 (used when bit 2 is set at 32749)
54850 | DEFB 251 | MSB of 64316 (used when bit 1 is set at 32749)
54851 | DEFB 114 | MSB of 29278 (used when bit 0 is set at 32749)