| Data

54332: MSBs of addresses of ERIC-handling routines

Used by the routine at 63405. The corresponding LSBs can be found at 54076.
54332 | DEFB 242 | MSB of 62094 (used when bit 7 is set at 32763)
54333 | DEFB 0 | Unused (when bit 6 is set at 32763, ERIC is incapacitated)
54334 | DEFB 94 | MSB of 24237 (used when bit 5 is set at 32763)
54335 | DEFB 94 | MSB of 24175 (used when bit 4 is set at 32763)
54336 | DEFB 225 | MSB of 57669 (used when bit 3 is set at 32763)
54337 | DEFB 242 | MSB of 62178 (used when bit 2 is set at 32763)
54338 | DEFB 0 | Unused (when bit 1 is set at 32763, ERIC's secondary status flags at 32749 are checked)
54339 | DEFB 93 | MSB of 23907 (used when bit 0 is set at 32763)