| Data

C100: Character buffer for little boy no. 4 (0xC1)

See the character buffer documentation for details of how bytes 0x00-0x1F of the buffer are used. This character's personal timetable follows at C125.
C100 | DEFS $20 |
C120 | DEFB $C0 | Initial animatory state: 0xC0 (see F5BE)
C121 | DEFB $48,$11 | Initial location (see F5BE)
C123 | DEFB $00 | Initial flags for byte 0x1D (see F5BE)
C124 | DEFB $2A | Random location table identifier (see 64D7)