| Routines

693D: Print a speech bubble UDG

Used by the routine at 694E.
Input
DE | UDG address
HL | Attribute file address
693D | PUSH HL | Save the attribute file address temporarily
693E | LD (HL),$38 | INK 0: PAPER 7
6940 | LD A,H | Set HL to the corresponding display file address
6941 | AND $0B
6943 | ADD A,A
6944 | ADD A,A
6945 | ADD A,A
6946 | LD H,A
6947 | EX DE,HL |
6948 | CALL $6125 | Copy the speech bubble UDG onto the screen
694B | EX DE,HL |
694C | POP HL | Restore the attribute file address to HL
694D | RET |