| Data

C700: Character buffer for little boy no. 10 (0xC7)

See the character buffer documentation for details of how bytes 0x00-0x1F of the buffer are used. This character's personal timetable follows at C725.
C700 | DEFS $20 |
C720 | DEFB $C0 | Initial animatory state: 0xC0 (see F5BE)
C721 | DEFB $7E,$11 | Initial location (see F5BE)
C723 | DEFB $00 | Initial flags for byte 0x1D (see F5BE)
C724 | DEFB $2C | Random location table identifier (see 64D7)