| Data

54588: LSBs of addresses of ERIC-handling routines

Used by the routine at 63405. The corresponding MSBs can be found at 54844.
54588 | DEFB 22 | LSB of 29462 (used when bit 7 is set at 32749)
54589 | DEFB 35 | LSB of 23843 (used when bit 6 is set at 32749)
54590 | DEFB 51 | LSB of 23859 (used when bit 5 is set at 32749)
54591 | DEFB 204 | LSB of 64460 (used when bit 4 is set at 32749)
54592 | DEFB 160 | LSB of 64416 (used when bit 3 is set at 32749)
54593 | DEFB 3 | LSB of 64259 (used when bit 2 is set at 32749)
54594 | DEFB 60 | LSB of 64316 (used when bit 1 is set at 32749)
54595 | DEFB 94 | LSB of 29278 (used when bit 0 is set at 32749)