| Routines

31905: Lower the signal for a certain event (unused)

This routine is not used.
Input
H | Character number (183-209)
31905 | CALL 25213 | Get the next byte (the event ID) from the command list
31908 | CALL 31861 | Convert the event ID into an appropriate bit mask
31911 | CPL | Set all but the event bit
31912 | AND (HL) | Merge the existing event flags, keeping the event bit reset
31913 | JR 31900 | Reset the appropriate bit at 32640 or 32641