| Data

BA00: Character buffer for little girl no. 4 (0xBA)

See the character buffer documentation for details of how bytes 0x00-0x1F of the buffer are used. This character's personal timetable follows at BA25.
BA00 | DEFS $20 |
BA20 | DEFB $C8 | Initial animatory state: 0xC8 (see F5BE)
BA21 | DEFB $A0,$11 | Initial location (see F5BE)
BA23 | DEFB $00 | Initial flags for byte 0x1D (see F5BE)
BA24 | DEFB $26 | Random location table identifier (see 64D7)