| Data

D43C: MSBs of addresses of ERIC-handling routines

Used by the routine at F7AD. The corresponding LSBs can be found at D33C.
D43C | DEFB $F2 | MSB of F28E (used when bit 7 is set at 7FFB)
D43D | DEFB $00 | Unused (when bit 6 is set at 7FFB, ERIC is incapacitated)
D43E | DEFB $5E | MSB of 5EAD (used when bit 5 is set at 7FFB)
D43F | DEFB $5E | MSB of 5E6F (used when bit 4 is set at 7FFB)
D440 | DEFB $E1 | MSB of E145 (used when bit 3 is set at 7FFB)
D441 | DEFB $F2 | MSB of F2E2 (used when bit 2 is set at 7FFB)
D442 | DEFB $00 | Unused (when bit 1 is set at 7FFB, ERIC's secondary status flags at 7FED are checked)
D443 | DEFB $5D | MSB of 5D63 (used when bit 0 is set at 7FFB)