| Routines

5EB7: Signal that ERIC is firing the catapult, hitting, or kissing

Used by the routines at 5EC7, 5EE8 and 5F1C.
Input
A | ERIC's next animatory state (bit 7 reset)
5EB7 | LD HL,$7FF3 | Initialise ERIC's main action timer at 7FF3 to 5
5EBA | LD (HL),$05
5EBC | LD L,$FB | HL=7FFB (ERIC's status flags)
5EBE | LD (HL),$20 | Set bit 5: ERIC is firing, hitting or kissing
5EC0 | POP HL | HL=address of the instruction after the CALL 5EB7 that got us here; store this at 7FD7 for collection later by the routine at 5EAD
5EC1 | LD ($7FD7),HL
5EC4 | JP $E132 | Begin the fire/hit/kiss action