| Messages

7F8A: Message 5: '{lines recipient}/combination number or letter/{room}'

Used by the routines at 7414 (as a submessage of message 0x0D), 74C8 (as a submessage of message 0x0E) and 7EB1 (as a submessage of message 0x10).
7F8A | DEFB $00 | The message number of the lines recipient (0x1B, 0x1C, 0x1D, 0x1E, 0x1F), the combination letter/number, or the room message number (0x80, 0x81, 0x82, 0x83, 0x84, 0x85, 0x86) goes here
7F8B | DEFB $00 | End marker