| Routines

61624: Restart the command list

Used by the routines at 62572 and 63501, and by command lists 18, 28, 30, 42, 44, 64, 66, 68, 70 and 78.
Input
H | Character number (183-209)
61624 | LD L,29 | Set bit 0 of byte 29 of the character's buffer, indicating to the routine at 25296 that the command list should be restarted
61626 | SET 0,(HL)
61628 | JP 25484 | Move to the next command in the command list (which will be the first command)