| Data

54076: LSBs of addresses of ERIC-handling routines

Used by the routine at 63405. The corresponding MSBs can be found at 54332.
54076 | DEFB 142 | LSB of 62094 (used when bit 7 is set at 32763)
54077 | DEFB 0 | Unused (when bit 6 is set at 32763, ERIC is incapacitated)
54078 | DEFB 173 | LSB of 24237 (used when bit 5 is set at 32763)
54079 | DEFB 111 | LSB of 24175 (used when bit 4 is set at 32763)
54080 | DEFB 69 | LSB of 57669 (used when bit 3 is set at 32763)
54081 | DEFB 226 | LSB of 62178 (used when bit 2 is set at 32763)
54082 | DEFB 0 | Unused (when bit 1 is set at 32763, ERIC's secondary status flags at 32749 are checked)
54083 | DEFB 99 | LSB of 23907 (used when bit 0 is set at 32763)