| Unused

40442: Unused

40442 | DEFS 2 |
If the following bytes were used, they would be the entry for phase 7+ in the water animation table (see the entry for phase 6+ at 40188, and the routine at 63915).
40444 | DEFB 124 | 124: water fired from pistol (phase 5+)
40445 | DEFB 0 | 0: x-coordinate increment
40446 | DEFB 1 | +1: y-coordinate increment
40447 | DEFB 2 | 2=may hit a plant or the ground at this phase