| Data

D63C: MSBs of addresses of ERIC-handling routines

Used by the routine at F7AD. The corresponding LSBs can be found at D53C.
D63C | DEFB $73 | MSB of 7316 (used when bit 7 is set at 7FED)
D63D | DEFB $5D | MSB of 5D23 (used when bit 6 is set at 7FED)
D63E | DEFB $5D | MSB of 5D33 (used when bit 5 is set at 7FED)
D63F | DEFB $FB | MSB of FBCC (used when bit 4 is set at 7FED)
D640 | DEFB $FB | MSB of FBA0 (used when bit 3 is set at 7FED)
D641 | DEFB $FB | MSB of FB03 (used when bit 2 is set at 7FED)
D642 | DEFB $FB | MSB of FB3C (used when bit 1 is set at 7FED)
D643 | DEFB $72 | MSB of 725E (used when bit 0 is set at 7FED)