| Routines

28558: Make ANGELFACE throw a punch (2)

The address of this uninterruptible subcommand routine is placed into bytes 111 and 112 of ANGELFACE's buffer by the routine at 28544.
Input
H | 168 (ANGELFACE)
28558 | LD L,111 | Place the address of the uninterruptible subcommand routine at 28642 into bytes 111 and 112 of ANGELFACE's buffer
28560 | LD (HL),226
28562 | CALL 25108 | Update the SRB for ANGELFACE's current animatory state
28565 | INC A | A=43/171: ANGELFACE hitting (phase 2)
28566 | CALL 25008 | Update ANGELFACE's animatory state and update the SRB, then continue into the routine at 28569