| Routines

6B32: Send a character on a mini-walkabout

The address of this primary command routine is placed into bytes 0x63 and 0x64 of a character's buffer by the routine at 6B3D. It either sends the character to his next walkabout destination (the walkabout origin or some spot within 7 spaces to the left of it), or moves to the next command in the command list if the designated number of walkabouts has been completed.
Input
H | Character number (0x98-0xA9)
6B32 | LD L,$67 | Decrement the walkabouts counter in byte 0x67 of the character's buffer
6B34 | DEC (HL)
6B35 | JP Z,$62A8 | Move to the next command in the command list if all the walkabouts have been done
6B38 | JP $62E5 | Otherwise go for another mini-walkabout