| Routines

27442: Send a character on a mini-walkabout

The address of this primary command routine is placed into bytes 99 and 100 of a character's buffer by the routine at 27453. It either sends the character to his next walkabout destination (the walkabout origin or some spot within 7 spaces to the left of it), or moves to the next command in the command list if the designated number of walkabouts has been completed.
Input
H | Character number (152-169)
27442 | LD L,103 | Decrement the walkabouts counter in byte 103 of the character's buffer
27444 | DEC (HL)
27445 | JP Z,25256 | Move to the next command in the command list if all the walkabouts have been done
27448 | JP 25317 | Otherwise go for another mini-walkabout