| Data

75A3: Lines bubble edge graphics

Used by the routine at 75B4. The graphic bytes are arranged in eight pairs. The first byte (after 1 is added to the value) of each pair corresponds to the left edge of the lines bubble, and the second byte corresponds to the right edge.
| Left edge
| Right edge
75A3 | DEFB $7F,$01 |
75A5 | DEFB $BF,$03 |
75A7 | DEFB $DF,$07 |
75A9 | DEFB $EF,$0F |
75AB | DEFB $EF,$0F |
75AD | DEFB $DF,$07 |
75AF | DEFB $BF,$03 |
75B1 | DEFB $7F,$01 |
75B3 | DEFB $FF | End marker