| Routines

31178: Control EINSTEIN during class (2)

The address of this primary command routine is placed into bytes 99 and 100 of EINSTEIN's buffer by the routine at 31162. After EINSTEIN has finished speaking, control resumes here.
Input
H | 169 (EINSTEIN)
31178 | LD L,99 | Replace the address of this primary command routine in bytes 99 and 100 of EINSTEIN's buffer with that of 31162
31180 | LD (HL),186
31182 | LD HL,32713 | 32713 holds the lesson signal flags
31185 | RES 7,(HL) | Signal: EINSTEIN has just spoken (so it's now the teacher's turn to speak)
31187 | RET |