| Game status buffer

7F0C: Screen refresh buffer (SRB)

Used by the routines at 6980, 6992, 7087, 72D2 and 7427. Each byte of the SRB corresponds to a segment of 8 character squares on the screen, the leftmost of which will be at x=0, x=8, x=16 or x=24. Each bit set in an SRB byte corresponds to a character square in the segment that needs refreshing. Bit 0 corresponds to the leftmost character square in the segment, bit 7 to the rightmost character square.
7F0C | DEFS $54 |