| Data

688C: Keypress vector table for keyboard input

Used by the routine at 68A0. These 10 bytes are copied to 6830 in the keypress offset table (the entries for keys 0-9) if Int2 is not selected.
688C | DEFB $89 | 0: Fire catapult
688D | DEFB $00 | 1: Unused
688E | DEFB $00 | 2: Unused
688F | DEFB $00 | 3: Unused
6890 | DEFB $00 | 4: Unused
6891 | DEFB $09 | 5: Move left (fast)
6892 | DEFB $06 | 6: Move down (fast)
6893 | DEFB $03 | 7: Move up (fast)
6894 | DEFB $0C | 8: Move right (fast)
6895 | DEFB $00 | 9: Unused