| Routines

76F9: Print the score, lines total or hi-score (2)

Continues from 76C8. Checks whether ERIC is over the lines limit (if the number of lines was just printed).
Input
DE | Display file address: 51BC (score), 51DC (lines) or 51FC (hi-score)
76F9 | LD A,E | Copy the LSB of the display file address to A
76FA | CP $DC | Was it the lines total that was just printed?
76FC | RET NZ | Return if not
76FD | JP $F9BB | Otherwise check whether ERIC is over the lines limit