| Routines

1C4E: THE 'COMMAND CLASS +02' ROUTINE

The address of this routine is derived from an offset found in the command class table. Command class +02 is concerned with the actual calculation of the value to be assigned in a LET statement.
CLASS_02 | 1C4E | POP BC | The address SCAN_LOOP is dropped.
| 1C4F | CALL VAL_FET_1 | The assignment is made.
| 1C52 | CALL CHECK_END | Move on to the next statement either via CHECK_END if checking syntax, or STMT_RET if in 'run-time'.
| 1C55 | RET