| Routines

10411: THE 'FUNCTION SKIPOVER' SUBROUTINE

This subroutine is used by S_FN_SBRN and by STK_F_ARG to move HL along the DEF FN statement while leaving CH-ADD undisturbed, as it points along the FN statement.
Input
HL | Address of the current character
Output
A | Code of next non-control, non-space character
HL | Address of that character
FN_SKPOVR | 10411 | INC HL | Point to the next code in the statement.
| 10412 | LD A,(HL) | Copy the code to A.
| 10413 | CP 33 | Jump back to skip over it if it is a control code or a space.
| 10415 | JR C,FN_SKPOVR
| 10417 | RET | Finished.